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Our range of Reinforced Polymer Composite (RPC) Manhole
Covers, engineered in accordance with EN124 standards.

EN124-B125
Suitable for pedestrian areas, footpaths, and parking zones
with light traffic.

Load Bearing Capacity: 12.5 Tons

EN124-C250
|deal for kerbside channels and areas with moderate vehicular
traffic.

Load Bearing Capacity: 25 Tons
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EN124-D400
Designed for carriageways, roads, and heavy-duty traffic areas.
Load Bearing Capacity: 40 Tons
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1.5 km kahna kacha
Road, Lahore.





